NOT A BID FORM


PROPOSAL TO SUMMIT TOWNSHIP WATER AUTHORITY
FOR HERSHEY ROAD WATER INFRASTRUCTURE REPLACEMENT PROJECT
(Note: Summit Township Water Authority Has Purchased All Waterline Materials)

PROJECT NO. 0000034086

	REF NO.
	DESCRIPTION – BASE BID
	QTY
	MEASURE
UNIT

	1. 
	12” Class 52 D.I. Waterline and Fittings (AWWA C111 Joints and Thrust Blocks)
	8,306
	L.F.

	2. 
	6” Class 52 D.I. Waterline and Fittings (AWWA C111 Joints and Thrust Blocks)
	40
	L.F.

	3. 
	V-Bio Polywrap, 6” and 12”
	8,346
	L.F.

	4. 
	6” Base Hydrant Assembly with 6” Valve
	12
	Each

	5. 
	6” M.J. Resilient Wedge Gate Valve
	1
	Each

	6. 
	8” M.J. Resilient Wedge Gate Valve
	2
	Each

	7. 
	12” M.J. Resilient Wedge Gate Valve
	22
	Each

	8. 
	Service Connections (Corp Stop, Curb Stop, Curb Box)
	92
	Each

	9. 
	Relocated Water Meter Pit, per Detail
	2
	Each

	10. 
	Air Release Manhole, per Detail
	5
	Each

	11. 
	Stream Crossing Manhole w/ Handwheel Valve, per Detail.
	2
	Each

	12. 
	20” Steel Casing Sleeve, per Detail
	145
	L.F.

	13. 
	Pipe Embedment, per CL B Pipe Embedment Detail.
	2,100
	Cu. Yd.

	14. 
	Asphalt Restoration, per Detail
	236
	S.Y.

	15. 
	Concrete Restoration, per Detail
	1,325
	S.F.

	16. 
	6” Gravel Restoration (Limestone)
	15
	Cu. Yd.

	17. 
	Lawn Restoration
	37,426
	S.F.

	18. 
	Landscape Restoration
	1
	Each

	19. 
	Bonds and Insurances
	1
	Each

	20. 
	Maintenance of Traffic
	1
	Each

	21. 
	Testing
	1
	Each











