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	ITEM
	DESCRIPTION
	QTY
	UNIT

	1
	Mobilization / Demobilization
	1
	LS

	
2
	Furnish and install complete, 8-inch C900 Waterline
	
1,900
	
LF

	
3
	Furnish and install complete, 8-inch C900 Waterline (RJ) with 16-inch Steel Casing
	
80
	
LF

	
4
	Furnish and install complete, 8-inch Gate Valves
	
2
	
EA

	
5
	Furnish and install complete, 6-inch Gate Valves
	
6
	
EA

	
6
	Furnish and install complete, 6-inch Hydrant
	
1
	
EA

	7
	Furnish and install complete, Tracer Wire
	1,980
	LF

	8
	Connection to existing
waterline, complete, as per plan
	2
	LS

	
9
	Type F Pavement Replacement w/ Compacted Granular
Backfill
	
133
	
SY

	
10
	Type C Pavement Replacement w/ Low Strength Mortar Backfill
	
15
	
SY

	
11
	Type C Pavement Replacement w/ Compacted Granular Backfill
	
200
	
SY

	12
	Seeding and Mulching
	1
	LS



